ABC Widget Oilfield Services Ltd. - FORMAL HAZARD ASSESSMENT

**Task Assessed:** Operate Forklift – loading and unloading

**Positions Considered:** Shop & Field super, welder, machinist, Labourer, field tech

**Assessment Team:** *(needs to include affected employee)*

### John Downy; Kris Marsh; Blake Edwards, Arthur Curry, Sandra Bullox

**Date:** Nov. 1, 2018

**FHA #:** # 011

# Revision #: 1

**Referenced Legislation:**

OH&S Code: Part 19 -8 – Powered Mobile Equipment Part 6-9; 6-1- Cranes Hoist &

Lifting Devices; Part 21- Rigging

# Specialized PPE or Equipment:

### anti slip boots

Severity

1. Negligible/OK: Causing minor injury that requires first aid or less
2. Minor: Causing non-serious injury, illness, or damage that requires medical aid
3. Serious: Causing severe injury, serious illness, that is dis- abling or lifelong, or property and equipment damage
4. Imminent danger: Causing death, widespread occupa- tional illness, or loss of facilities

Probability

1. Extremely Remote: Unlikely to occur
2. Remote: Could occur at some point
3. Reasonably Probable: Likely to occur eventu- ally
4. Probable: Likely to occur immediately or soon

## Hazards Associated with Task

## Existing Hazard Controls

Outstanding Implementation Assigned To

## Expected Completion Date

Unintentional contact with personnel

Severity

Probability

Priority

Severity

Probability

Priority

Unintentional contact with truck

4 4 16

2 4 8

Eng: adequate lighting

Admin: SJP # 011; Training, back-up alarm, PM (lights and brakes), speed limit PPE: Boots

Eng: adequate exterior lighting

Admin: SJP # 011; Training, PM (lights and brakes), speed limit

PPE:

4 2 8

1 3 3

## Hazards Associated with Task

Existing Hazard Controls

Outstanding Implementation Assigned To

Expected Completion Date

Load stability (in motion)

Severity

Probability

Priority

Probability

Priority

Materials Falling Off Truck

Awkward load (generally unstable)

Uneven Ground/ Ice

Low Visibility

3 4 12

3 4 12

3 4 12

4 4 16

4 4 16

Eng:

Severity

Admin: SJP # 010; Training, speed limit, fork positioning, proper tool selection

3

PPE:

Eng:

Admin: SJP # 010; enforced safe work zone 3

PPE: boots

Eng:

Admin: SJP # 010; spotter, square on forks, speed limit, weight limit scale followed PPE:

3

Eng: tire chains (when appropriate)

Admin: SJP # 008; Training, speed limit, 4

regular grading of yard

PPE: anti slip boots

Eng: adequate yard lighting, FL lights Admin: SJP # 008; Training, speed limit,

PM of lights and brakes, back-up alarm 4

PPE:

3 9

3 9

3 9

3 12

3 12